


Legacy Flight Performance Testing

30 July 2019

Version 1.5



645 Colonel Glenn Blvd

Dayton, Ohio

DISCLAIMER: This document has been produced to support training and experimentation ONLY. It does not represent any system, real or planned. No United States Government resources were used to produce this document.

**THIS PAGE IS INTENTIONALLY BLANK**

Contents

[1. Introduction 5](#_Toc28791148)

[2. Flight Performance 5](#_Toc28791149)

[2.1. Test 01-01 5](#_Toc28791150)

[2.1.1. Maximum Airspeed 5](#_Toc28791151)

[2.1.2. Maximum Altitude 6](#_Toc28791152)

[2.1.3. Time to Climb 6](#_Toc28791153)

[2.2. Test 01-02 6](#_Toc28791154)

[2.3. Test 01-03 7](#_Toc28791155)

[3. Control Communications 8](#_Toc28791156)

[3.1. Test 02-01 8](#_Toc28791157)

[3.1.1. Control Link Operational Range 8](#_Toc28791158)

[3.1.2. Lost Link Detection and Behavior 8](#_Toc28791159)

[4. Navigation 9](#_Toc28791160)

[4.1. Test 03-01 9](#_Toc28791161)

[4.1.1. Stationary Error 9](#_Toc28791162)

[4.1.2. Moving Error 9](#_Toc28791163)

**THIS PAGE IS INTENTIONALLY BLANK**

1. Introduction

The Nomad system is based heavily on the legacy Wanderer UAV system, to the extent that all relevant flight performance characteristics are identical to the previous variant. A key part of XYZ’s competitive offering is the fact that no major flight performance re-designs were required to adapt the basic Wanderer vehicle to meet the OTSS-E requirements. Because of this, XYZ was able to execute an expedited flight test program using the previous Wanderer flight test article (known as Wanderer Baseline, or Wanderer-01). This article was designed with the ability to ballast as needed to emulate the various Wanderer configurations. The anticipated Nomad configurations fall within the range of existing Wanderer variants, and as such has been extensively tested. To confirm this, XYZ performed a limited series of tests to confirm the flight performance with the exact design parameters of the final Nomad configuration. These tests were conducted over 3 days (10-12 July 2019) using a legacy ground station.

1. Flight Performance
   1. Test 01-01

Test 01-01 was designed to test the basic flight performance capability of the Nomad configuration. Test 01-01 consisted of 3 test points; maximum airspeed, maximum altitude and time to climb. Test 01-01 was conducted on 10 July 2019 in Dayton, Ohio. All testing was conducted within line of site of the operator.

|  |  |
| --- | --- |
| Test 01-01 Metadata |  |
| Date | 10 July 2019 |
| Location | Dayton, Ohio |
| Altitude | 900 ft MSL |
| Configuration | Wanderer-01-01 |
| Weight | 27.5 lbs |
| Xcg | 0.75 in |
| Ycg | 0.15 in |
| Zcg | 1.20 in |

* + 1. Maximum Airspeed

The first test point of Test 01-01 tested the maximum airspeed of the system. The test was conducted by flying forward (in relation to the drone) at maximum speed.

|  |  |
| --- | --- |
| Test 01-01-01 |  |
| Time | 1400L |
| Temperature | 78 deg F |
| Windspeed | 0 knots |
| Maximum Airspeed | 32.15 mph |

* + 1. Maximum Altitude

Test point 01-01-02 tested the maximum altitude that the system could attain. The test was executed by climbing at a consistent power setting until the vertical velocity reached zero, then increasing power. Testing continued until zero velocity was achieved while using maximum thrust. The vehicle then maintained this altitude for 5 seconds before making a controlled descent.

|  |  |
| --- | --- |
| Test 01-01-02 |  |
| Time | 1500L |
| Temperature | 81 deg F |
| Windspeed | 0 knots |
| Maximum Altitude | 1500 ft MSL |

* + 1. Time to Climb

Test point 01-01-03 tested how fast the vehicle could climb to 100 ft AGL. To accomplish this, the vehicle was powered on at 0 altitude and the maximum power was applied until the vehicle reached 100 ft AGL.

|  |  |
| --- | --- |
| Test 01-01-03 |  |
| Time | 1600L |
| Temperature | 75 deg F |
| Windspeed | 0 knots |
| Initial Altitude | 900 ft MSL |
| Final Altitude | 1000 ft MSL |
| Elapsed Time | 18 seconds |

* 1. Test 01-02

Test 01-02 tested the systems endurance. Testing was completed within line of system of the ground station by flying the vehicle in a circle until the system battery reached 2% (minimum safe landing condition). Testing was conducted by flying at 125 feet AGL.

|  |  |
| --- | --- |
| Test 01-02 Metadata |  |
| Date | 11 July 2019 |
| Location | Dayton, Ohio |
| Altitude | 900 ft MSL |
| Configuration | Wanderer-01-01 |
| Weight | 27.5 lbs |
| Xcg | 0.75 in |
| Ycg | 0.15 in |
| Zcg | 1.20 in |

|  |  |
| --- | --- |
| Test 01-02-01 |  |
| Time | 1000L |
| Temperature | 65 deg F |
| Mission Endurance | 23 minutes |

* 1. Test 01-03

Test 01-03 tested the control capability of the vehicle. Testing was conducted using a legacy ground station; however, the control messages and control link were identical to the final Nomad configuration. All testing was conducted within line of site of the operator.

|  |  |
| --- | --- |
| Test 01-03 Metadata |  |
| Date | 11 July 2019 |
| Location | Dayton, Ohio |
| Altitude | 900 ft MSL |
| Configuration | Wanderer-01-01 |
| Weight | 27.5 lbs |
| Xcg | 0.75 in |
| Ycg | 0.15 in |
| Zcg | 1.20 in |

During Test 01-03, the control capability of the vehicle was demonstrated. For lateral speed control, the system has to different operational modes: (1) direct control of thrust vector, and (2) speed hold mode. In direct control mode, the user manipulates the control stick, and the angle and magnitude of lateral thrust is updated. As this happens, the vehicle automatically maintains the selected flight path angle, adjusting the angle of attack as needed. Assuming pitch and roll inputs are neutral (0 degrees commanded), the flight path angle will be 0 and the vehicle will maintain a constant altitude. In speed hold mode, the user selects the lateral speed using the control stick, and the presses the speed hold button. The vehicle will then maintain the selected speed and flight path angle, adjust thrust, roll and pitch as needed.

To control roll and pitch, the user manually controlled the vehicle flight path angle. As the control stick moved further from neutral, the vehicle increased the target flight path angle up to a maximum of 45 degrees at maximum control deflection. Roll and pitch rate were determined by two factors: (1) speed the stick changed position, and (2) control limits built into the software. When the stick was released, the vehicle returned to steady level flight. Yaw control behaved differently: the yaw controls commanded yaw rate, rather than angle. As the control triggers were depressed, the yaw rate increased up to a maximum of 20 degrees per second. If both triggers were depressed simultaneously, then the resulting yaw rate equaled the difference between the two commands, down to 0 degrees per second if both were depressed equally. When the controls were released, the yaw rate returned to zero, enabling movement along a consistent heading without yaw input.

1. Control Communications
   1. Test 02-01

Test 01-03 was design to test the control communications system, including the operational range and the lost link capability.

|  |  |
| --- | --- |
| Test 02-01 Metadata |  |
| Date | 11 July 2019 |
| Location | Springfield, Ohio |
| Altitude | 900 ft MSL |
| Configuration | Wanderer-01-01 |
| Weight | 27.5 lbs |
| Xcg | 0.75 in |
| Ycg | 0.15 in |
| Zcg | 1.20 in |

* + 1. Control Link Operational Range

Test point 02-01-01 was designed to test the control link operational range. To accomplish this, testing was moved to Springfield, Ohio where additional range space was available. Testing consisted of flying the vehicle directly away from the ground station at a constant speed and altitude (300 feet AGL). During this time, the vehicle moved outside of visual range of the ground station. Positive visual control was maintained by helicopter.

|  |  |
| --- | --- |
| Test 02-01-01 |  |
| Time | 1500L |
| Temperature | 75 deg F |
| Ground Range to Base station | 12 miles |

* + 1. Lost Link Detection and Behavior

To test lost link detection, the vehicle was flown to 300 feet AGL and the control link was physically disabled at the ground station. Prior to takeoff, the battery was discharged to 15%, ensuring that the vehicle would remain on the test range if unanticipated behavior occurred. The vehicle remained within line of site during the entire test.

The tests showed that the vehicle successfully detected when the link was disabled, with a latency of 5 seconds. This delay was intentional to account for intermittent communications outages. Upon detection of link loss, the vehicle entered a stable hover at the target altitude. When link was re-enabled, the vehicle detected, authenticated and re-established full control. When the link remained in-operational, the vehicle maintained hover until battery life was calculated at less than 5 minutes, upon which the vehicle initiated a controlled descent.

1. Navigation
   1. Test 03-01

Test 03-01 tested the basic navigation accuracy of the legacy Wanderer system.

|  |  |
| --- | --- |
| Test 03-01 Metadata |  |
| Date | 12 July 2019 |
| Location | Dayton, Ohio |
| Altitude | 900 ft MSL |
| Configuration | Wanderer-01-01 |
| Weight | 27.5 lbs |
| Xcg | 0.75 in |
| Ycg | 0.15 in |
| Zcg | 1.20 in |

* + 1. Stationary Error

During testing, the legacy Wanderer navigation system showed less than expected performance, especially during stationary testing where the inertial navigation capability could not be effectively utilized. Testing was conducted by holding the vehicle steady at a constant altitude (300 ft AGL).

|  |  |
| --- | --- |
| Test 03-01-01 |  |
| Time | 1400L |
| Temperature | 75 deg F |
| Latitude Error | 11 ft |
| Longitude Error | 11 ft |
| Altitude Error | 15 ft |
| Absolute velocity | 0.1 ft/s |

* + 1. Moving Error

Test point 03-01-02 showed that combining the inertial capability with the GPS improved accuracy, but not enough to meet the originating requirements. Testing was conducted by moving at a constant velocity (2.5 ft/s) at a constant altitude (300 ft AGL).

|  |  |
| --- | --- |
| Test 03-01-02 |  |
| Time | 1500L |
| Temperature | 75 deg F |
| Latitude Error | 7 ft |
| Longitude Error | 7 ft |
| Altitude Error | 10 ft |
| Absolute velocity | 2.5 ft/s |